# Print and release checklist

## Recommended first print

Print the Standard 6-slot model first:

`models/SHIRE3D_Cable_Valet_6_Slot.stl`

## Starting profile

- Material: PLA or PETG
- Layer height: 0.20 mm
- Walls: 3
- Top and bottom layers: 4
- Infill: 15% gyroid
- Supports: Off
- Orientation: Flat base on build plate
- Brim: Normally unnecessary

## Required physical checks

- All cable slots accept common charging leads without cutting or pinching them.
- Cables remain retained during normal desk use.
- Tray has no sharp edges or print defects.
- Base sits flat without rocking.
- Label recess prints cleanly.
- Product survives repeated cable insertion and removal.
- Actual print time and filament use are recorded from the slicer.
- Listing photographs show the real printed product.
- Ray approves the final version before publishing.
